This program implements the cochannel speech separation algorithm described in "An iterative model-based approach to cochannel speech separation," by K. Hu and D. L. Wang, 2012 (submitted to IEEE Trans. Audio, Speech, and Lang. Process.)

The MATLAB program run/twoSpeaker.m is a wrapper including several related model-based algorithms. The core separation algorithms are written in C++ under folder “c”.

**Usage**:

rmask = twoSpeaker(sig, sid, type, nGau, bW, snr\_criterion, nStep, workFolder)

**Inputs:**

sig: Input time-domain cochannel speech signal

sid: Two speaker identities (sid(1) and sid(2))

type: 'acoustDym\_iter' – The iterative model-based algorithm

'ReddyRaj' - Reddy & Raj'07 (training and test energy levels must match)

'MMSE' - Minimum mean square estimation

'MAP' - Maximum *a posteriori* estimation

'acoustDym' – With temporal dynamics

'MMSE\_iter' – MMSE + iterative estimation

'MAP\_iter' – MAP + iterative estimation

nGau: Number of Gaussians in GMM (use 256 in this code)

bW: Beam width in a Viterbi search (use 16; only used in HMM-based algorithms)

snr\_criterion: A threshold (in dB) on the absolute SNR difference to stop iterative estimation (use 0.5)

nStep: Maximum number of iterations (make sure iterative estimation will stop)

workFolder: Folder storing temporary files

**Outputs:**

rmask: Estimated soft masks for two speaker (mask{1} and mask{2})

**Run an example:**

In Linux, go to the “run” folder, start MATLAB, and input the following commands:

sig = load('sample/t11\_lwby6p\_m30\_lrwp2a.-9dB.val2') ;

rmask = twoSpeaker(sig, [11,30], 'acoustDym\_iter', 256, 16, .5, 3, '.');

**Run related model-based methods:**

sig = load('sample/t11\_lwby6p\_m30\_lrwp2a.-9dB.val2') ;

* Reddy & Raj'07 (Training and test signal levels must match):

rmask = twoSpeaker(sig, [11,30], 'ReddyRaj07', 256, -1, -1, -1, '.');

(-1 means no parameter needed)

* MMSE:  
   rmask = twoSpeaker(sig, [11,30], 'MMSE', 256, -1, -1, -1, '.');
* MAP:  
   rmask = twoSpeaker(sig, [11,30], 'MAP', 256, -1, -1, -1, '.');
* MAP + acoustic dynamics:  
   rmask = twoSpeaker(sig, [11,30], ‘acoustDym’, 256, 16, -1, -1, '.');
* MMSE + iterative:

rmask = twoSpeaker(sig, [11,30], 'MMSE\_iter', 256, -1, .5, 3, '.');

* MAP + iterative:

rmask = twoSpeaker(sig, [11,30], 'MAP\_iter', 256, -1, .5, 3, '.');

**Notes:**

* Speakers in this program come from the Speech Separation Challenge (SSC) corpus. Speaker identities are numbered from 1-34 following the definition in the SSC corpus. For example, sid=[1,2] means the target is speaker 1 and interferer is speaker 2
* This implementation is in the log-cochleagram domain using 128-channel gammatone filterbank
* Sampling frequency is 16 kHz